models: 6bbI.t3d
animations: 4 4 0 0 2 0 -1
animwheelprefix: wheel0
animdoorprefix: door0
endmodels

sounds:
curve: curve_en57.wav 100
wheel_clatter: 35.0 -8.36 wheel_hyperloop_1.wav -5.57 wheel_hyperloop_2.wav  5.57 wheel_hyperloop_3.wav 8.36 wheel_hyperloop_4.wav end
brake: en57-pisk.wav 100.0 1000.0 -1.0
derail: derail.wav 200
horn1: 20786_syrena_en57-1112_1.wav 20786_syrena_en57-1112_2.wav 20786_syrena_en57-1112_3.wav 1000
horn2: 20786_syrena_en57-1112_4.wav 20786_syrena_en57-1112_5.wav 20786_syrena_en57-1112_6.wav 1000
compressor: comp_hyperloop_1.wav comp_hyperloop_2.wav comp_hyperloop_3.wav 30
departuresignal: { soundbegin: signal_hyperloop_3.wav soundmain: signal_hyperloop_10.wav soundend: signal_hyperloop_7.wav placement: engine }
sand: sand_1.wav sand_2.wav sand_3.wav 15 
releaser: releaser_1.wav releaser_2.wav releaser_3.wav 15 
dooropen: { soundmain: door_open_hyperloop.wav placement: external }
doorclose: { soundmain: door_close_hyperloop.wav placement: external }
outernoise: {
 range: 130
 crossfade: 85
 sound0: silence1.wav pitch0: 0
 sound50: runningnoise_hyperloop_low.wav pitch50: 50
 sound200: runningnoise_hyperloop_high.wav pitch200: 200 
 sound500: outernoise_hyperloop.wav pitch500: 500 
 sound800: outernoise_hyperloop.wav pitch800: 800 
 sound1500: outernoise_hyperloop.wav pitch1500: 1500 
endsounds

internaldata:
ctrl: 20786_nastawnik_en57-1112.wav
reverserkey: 07]nastbocz0-1.wav
buzzer: buzzer_hyperloop.wav
tachoclock: hasler_hyperloop.wav
//switch: 20786_switch_en57-1112.wav
relay: rewerser_hyperloop.wav
pneumaticrelay: kran_nag_hyperloop.wav
//relay: { sound0: 2193_en57-stycznik_lin-wyl.wav sound1: 2193_en57-stycznik_lin-zal.wav sound3: 2193_en57-wal_poz-np.wav sound5: 2193_en57-wal_poz-np.wav sound7: 2193_en57-wal_poz-np.wav sound9: 2193_en57-wal_poz-np.wav sound11: 2193_en57-wal_poz-np.wav sound13: 2193_en57-wal_poz-np.wav sound15: 2193_en57-wal_poz-np.wav sound17: 2193_en57-wal_poz-np.wav sound2: 2193_en57-wal_poz-p.wav sound4: 2193_en57-wal_poz-p.wav sound6: 2193_en57-wal_poz-p.wav sound8: 2193_en57-wal_poz-p.wav sound10: 2193_en57-wal_poz-p.wav sound12: 2193_en57-wal_poz-p.wav sound14: 2193_en57-wal_poz-p.wav sound16: 2193_en57-wal_poz-p.wav sound18: 2193_en57-wal_poz-p.wav sounddec: 2193_en57-wal_poz-np.wav }
//shuntfield: { sound1: 2193_en57-wal_poz-p.wav sound2: 2193_en57-wal_poz-np.wav sound3: 2193_en57-wal_poz-p.wav }
couplerattach: couplerattach.wav
couplerdetach: couplerdetach.wav
dooropen: signal_hyperloop_9.wav
doorclose: signal_hyperloop_8.wav

pneumaticswitch: kran_nag_hyperloop.wav

brakesound: brake.wav 1.0 0.4 0.2 0.9   
slipperysound: brake-slipp.wav 2.0 0.2  
airsound: hiss.wav 1000.0 -0.1  
fadesound: fadesound_hyperloop.wav
runningnoise: {
 range: 30
 crossfade: 90
 sound0: silence1.wav pitch0: 0
 sound50: runningnoise_hyperloop_low.wav pitch50: 50
 sound100: runningnoise_hyperloop_medium.wav pitch100: 100
 sound200: runningnoise_hyperloop_high.wav pitch200: 200
 sound500: runningnoise_hyperloop_high.wav pitch500: 500
 sound800: runningnoise_hyperloop_high.wav pitch800: 800 
 sound1500: runningnoise_hyperloop_high.wav pitch1500: 1500 

mechspring: 100      0.02 0.2 0.2 0.03 0.15  0.02   0.01

cab1definition:   
-1.8 1.2 8.88 1.8 1.1 9.5
driver1pos:       
0.0 2.8 8.93
driver1sitpos:    
-0.85 2.43 8.92
cab1model: kabina_EN57Ib.t3d

cab2definition:   
0.0 2.815 3.114 0.0 2.815 3.114 
driver2pos:      
0.0 2.815 3.114
cab2model: korytarz.t3d 
	

mainctrl: { nastawnik rot -0.0460 0.0 0.08 sound0: signal_hyperloop_2.wav sound1: signal_hyperloop_4.wav sound2: signal_hyperloop_5.wav sound3: signal_hyperloop_4.wav sound4: signal_hyperloop_5.wav sound5: signal_hyperloop_14.wav sound6: signal_hyperloop_6.wav }
brakectrl: { kran rot 0.073 -0.15 0.15 sound-2: kran)hyperloop.wav sound01: kran)hyperloop.wav sound0: kran)hyperloop.wav sound1: kran)hyperloop.wav sound2: kran)hyperloop.wav sound3: kran)hyperloop.wav sound4: kran)hyperloop.wav sound5: kran)hyperloop.wav sound6: kran_nag_hyperloop.wav }
dirkey: { nawrotnik rot -0.05 0.01 0.15 soundinc: rewerser_hyperloop sounddec: signal_hyperloop_12.wav sound0: signal_hyperloop_11.wav }

main_sw:  wylszybki { rot -0.2 0 0.2 soundinc: signal_hyperloop_8.wav sounddec: signal_hyperloop_9.wav }
security_reset_bt: { zbijacz mov -0.005 0 0.2 soundinc: button_hyperloop_3_on.wav sounddec: button_hyperloop_3_of.wav }
fuse_bt: { odblprzeknadm rot -0.2 0 0.2 soundinc: button_hyperloop_3_on.wav sounddec: button_hyperloop_3_of.wav }
compressor_sw: { sprezarka rot -0.2 0 0.2 soundinc: signal_hyperloop_16.wav sounddec: signal_hyperloop_16.wav }
converter_sw: { przetwzal rot -0.2 0 0.2 soundinc: signal_hyperloop_12.wav sounddec: signal_hyperloop_13.wav }
converteroff_sw: { przetwwyl rot -0.2 0 0.2 soundinc: signal_hyperloop_15.wav sounddec: signal_hyperloop_12.wav }
pantfront_sw: { panttylnypodniesiony rot -0.2 0 0.2 soundinc: signal_hyperloop_11.wav sounddec: signal_hyperloop_7.wav }
pantrear_sw: { pantprzednipodniesiony rot -0.2 0 0.2 soundinc: signal_hyperloop_9.wav sounddec: signal_hyperloop_8.wav }
pantfrontoff_sw: { pantprzedniopuszcz rot -0.2 0 0.2 soundinc: signal_hyperloop_17.wav sounddec: signal_hyperloop_7.wav }
pantalloff_sw: { pantopuszcz mov -0.005 0 0.2 soundinc: button_hyperloop_3_on.wav sounddec: button_hyperloop_3_of.wav }
trainheating_sw: { ogrzewanie rot -0.2 0 0.2 soundinc: signal_hyperloop_11.wav sounddec: signal_hyperloop_12.wav }
radio_sw: { radio rot -0.2 0 0.2 soundinc: signal_hyperloop_13.wav sounddec: signal_hyperloop_15.wav }
upperlight_sw: { reflgorny rot -0.2 0 0.2 soundinc: signal_hyperloop_16.wav sounddec: signal_hyperloop_16.wav }
leftlight_sw: { refllewy rot -0.2 0 0.2 soundinc: signal_hyperloop_16.wav sounddec: signal_hyperloop_16.wav }
rightlight_sw: { reflprawy rot -0.2 0 0.2 soundinc: signal_hyperloop_16.wav sounddec: signal_hyperloop_16.wav }
leftend_sw: { lewyprzyc rot -0.2 0 0.2 soundinc: rewerser_hyperloop.wav sounddec: rewerser_hyperloop.wav }
rightend_sw: { prawyprzyc rot -0.2 0 0.2 soundinc: rewerser_hyperloop.wav sounddec: rewerser_hyperloop.wav }
dimheadlights_sw: { reflprzyc rot -0.2 0 0.2 soundinc: signal_hyperloop_14.wav sounddec: signal_hyperloop_1.wav }
antislip_bt: { klamka rot 0.02 0 0.3 soundinc: button_hyperloop_2_on.wav sounddec: button_hyperloop_2_of.wav }


hornlow_bt: { Plane64 rot 0.01 0 0.02 soundinc: button_hyperloop_1_on.wav sounddec: button_hyperloop_1_of.wav }
hornhigh_bt: { Plane63 rot 0.01 0 0.02 soundinc: button_hyperloop_2_on.wav sounddec: button_hyperloop_2_of.wav }
door_left_sw: { drzwilewe  rot -0.2 0 0.2 soundinc: signal_hyperloop_9.wav sounddec: signal_hyperloop_8.wav }
door_right_sw: { drzwiprawe rot -0.2 0 0.2 soundinc: signal_hyperloop_9.wav sounddec: signal_hyperloop_8.wav }
departure_signal_bt: { sygnodjazdu rot -0.2 0 0.2 soundinc: button_hyperloop_1_on.wav sounddec: button_hyperloop_1_of.wav }
instrumentlight_sw: { oswietlenieprzyz rot -0.18 0 0.3 soundinc: signal_hyperloop_11.wav sounddec: signal_hyperloop_12.wav }
cablight_sw: { oswietleniekab rot -0.18 0 0.3 soundinc: signal_hyperloop_13.wav sounddec: signal_hyperloop_12.wav }
tachometerd: wskpr rot 0.000572709 0.0 0  
HVcurrent: ampwn mov 0.000014875 0 0.3        
Hvoltage: voltwn mov 0.0000002031 0 0.3 
Lvoltage: aperniski rot -0.001607142 0.11444 0.5
brakepress: Cyl rot 0.73013699 0 0
pipepress: PrzGl rot 0.74193548 0 0
compressor: Zb rot 0.45146245 0 0
clock: analog  //na razie tylko taki moze byc

i-converteroff: przetw
i-diff_relay: przeknadm
i-motor_ovld: przeknadm
i-mainbreakeroff: szybki
i-resistors: opory
i-security_aware: { czuwak soundinc: signal_hyperloop_2.wav sounddec: signal_hyperloop_2.wav }
i-security_cabsignal: { shp soundinc: signal_hyperloop_2.wav sounddec: signal_hyperloop_2.wav }
i-reserve: rezerwa
i-door_left: drzwilewe
i-door_right: drzwiprawe
i-departure_signal: odjazd
i-instrumentlight: podsw
i-voltbrake: napiecienast
i-radio: radio-wl

cab0definition:
0.0 2.815 3.114 0.0 2.815 3.114
driver0pos:
0.0 2.815 3.114
//nazwa modelu korytarza
cab0model: korytarz.t3d
