models: 6bbII.t3d
animations: 4 4 0 0 2 0 -1
animwheelprefix: wheel0
animdoorprefix: door0
endmodels

sounds:
curve: curve_en57.wav 100
wheel_clatter: 35.0 -8.36 20786_wheel_en57_3.wav -5.57 20786_wheel_en57_4.wav  5.57 20786_wheel_en57_1.wav 8.36 20786_wheel_en57_2.wav end
brake: en57-pisk.wav 100.0 1000.0 -1.0
derail: derail.wav 200
horn1: 20786_en57-780_syrena_nisk_1.wav 20786_en57-780_syrena_nisk_2.wav 20786_en57-780_syrena_nisk_3.wav 1000
horn2: 20786_en57-780_syrena_wys_1.wav 20786_en57-780_syrena_wys_2.wav 20786_en57-780_syrena_wys_3.wav 1000
compressor: 4873_compressor_en57-start.wav 4873_compressor_en57.wav 4873_compressor_en57-stop.wav 50
departuresignal: en57_signal_start.wav en57_signal.wav en57_signal_stop.wav 50
sand: sand_1.wav sand_2.wav sand_3.wav 15 
releaser: releaser_1.wav releaser_2.wav releaser_3.wav 15 
dooropen: 20786_door_open_en71-026.wav
doorclose: 20786_door_close_en71-026.wav
endsounds 

internaldata:
ctrl: 20786_nastawnik_en57-1112.wav
reverserkey: 07]nastbocz0-1.wav
buzzer: 20786_bzyczek_en57-1112.wav
tachoclock: 20786_tacho_en57-1112.wav
switch: 20786_switch2_en57-1112.wav
relay: relay-en57.wav
pneumaticrelay: pneumaticrelay.wav
couplerattach: couplerattach.wav
couplerdetach: couplerdetach.wav
dooropen: 20786_switch2_en57-1112.wav
doorclose: 20786_switch2_en57-1112.wav
pneumaticswitch: 20786_pneumatic_swith_en57-1112.wav

brakesound: brake.wav 1.0 0 0.2 0.9   
slipperysound: brake-slipp.wav 2.0 0.2  
airsound: [1007]fvel6_brake_1.wav 5 -0.01  
airsound2: [1007]fvel6_unbrake_15db_1.wav 5 -0.01  
airsound3: [1007]fvel6_emergency_1.wav 5 -0.01  
runningnoise: 20786_running_noise_en71-026.wav 4.0 0.45 3.5 0.05

mechspring: 100      0.02 0.2 0.2 0.03 0.15  0.02   0.01

cab2definition:   
-1.8 1.2 -9.5 1.8 1.1 -8.88
driver2pos:      
0.0 2.8 -8.95
driver2sitpos:   
0.85 2.43 -8.92
cab2model: kabina_EN57IIb.t3d 

cab1definition:   
0.0 2.815 -3.114 0.0 2.815 -3.114 
driver1pos:      
0.0 2.815 -3.114
cab1model: korytarz.t3d
	
mainctrl: nastawnik rot -0.0460 0.0 0.08          
brakectrl: kran rot 0.0625 0.0625 0.15        
dirkey: nawrotnik rot -0.05 0.01 0.15
main_sw:  wylszybki rot -0.2 0 0.2                  
security_reset_bt: zbijacz mov -0.005 0 0.2                               
fuse_bt: odblprzeknadm rot -0.2 0 0.2                    
compressor_sw: sprezarka rot -0.2 0 0.2
converter_sw: przetwzal rot -0.2 0 0.2
converteroff_sw: przetwwyl rot -0.2 0 0.2
pantfront_sw: panttylnypodniesiony rot -0.2 0 0.2
pantrear_sw: pantprzednipodniesiony rot -0.2 0 0.2
pantfrontoff_sw: pantprzedniopuszcz rot -0.2 0 0.2
pantalloff_sw: pantopuszcz mov -0.005 0 0.2
trainheating_sw: ogrzewanie rot -0.2 0 0.2
radio_sw: radio rot -0.125 0 0.2
upperlight_sw: reflgorny rot -0.2 0 0.2
leftlight_sw: refllewy rot -0.2 0 0.2
rightlight_sw: reflprawy rot -0.2 0 0.2
leftend_sw: lewyprzyc rot -0.2 0 0.2
rightend_sw: prawyprzyc rot -0.2 0 0.2
instrumentlight_sw: oswietlenieprzyz rot -0.18 0 0.3
cablight_sw: oswietleniekab rot -0.18 0 0.3

door_left_sw: drzwiprawe  rot -0.125 0 0.2
door_right_sw: drzwilewe rot -0.125 0 0.2
departure_signal_bt: sygnalodjazdu rot -0.125 0 0.2

tachometer: wskpr rot 0.00572709 0.0 0  
HVcurrent: ampwn mov 0.00014875 0 0.3         
Hvoltage: voltwn mov 0.00002031 0 0.3 
Lvoltage: aperniski rot -0.001607142 0.11444 0.5
brakepress: Cyl rot 0.73013699 0 0
pipepress: PrzGl rot 0.74193548 0 0
compressor: Zb rot 0.45146245 0 0
clock: analog  

i-converteroff: przetw
i-diff_relay: przeknadm
i-motor_ovld: przeknadm
i-mainbreakeroff: szybki
i-resistors: opory
i-security_aware: czuwak
i-security_cabsignal: shp
i-reserve: rezerwa
i-door_left: drzwiprawe
i-door_right: drzwilewe
i-departure_signal: odjazd
i-instrumentlight: podsw
i-voltbrake: napiecienast
i-radio: ir-wl

cab0definition:
0.0 2.815 -3.114 0.0 2.815 -3.114
driver0pos:
0.0 2.815 -3.114
cab0model: korytarz.t3d
