models: 6da.t3d
animations: 4 0 0 4 2 0 -1
lowpolyinterior: 6da_interior.t3d
animwheelprefix: wheel0
endmodels

locations:
 tractionmotors: -3.736 3.788 end
 bogies: -3.736 3.788 end
endlocations

sounds:
wheel_clatter: 70 -5.044 wheel-heavy.wav -2.444 wheel-heavy.wav 2.426 wheel-heavy.wav 5.026 wheel-heavy.wav end
oilpump: 697_sm42-oilpump.wav
engine: {
 amplitudeoffset: 1.2
 amplitudefactor: 0.8
 range: 150
 crossfade: 100
 soundend: 697_sm42-stop.wav
 sound495: 697_sm42-idle-1.wav pitch495: 495
 sound610: 697_sm42-idle-2.wav pitch610: 610
 sound710: 697_sm42-idle-3.wav pitch710: 710
 sound815: 697_sm42-idle-4.wav pitch815: 815
 sound930: 697_sm42-idle-5.wav pitch930: 912
 sound1100: 697_sm42-idle-5.wav pitch1100: 1040 }
tractionmotor: 697_st44-motor.wav 10.0  1.5 0.8  0.16 0.1
turbo: {
 frequencyfactor: 2.0
 frequencyoffset: -1.5
 range: 50
 soundmain: 697_sm42-turbo.wav }
brake: 697_sm42_brake.wav 100.0 1700.0 -1.0
derail: derail.wav 200
horn1: 697_sm42-horn1-start.wav 697_sm42-horn1-trwa.wav 697_sm42-horn1-stop.wav 1000 
horn2: 697_sm42-horn2-start.wav 697_sm42-horn2-trwa.wav 697_sm42-horn2-stop.wav 1000 
sand: sand_1.wav sand_2.wav sand_3.wav 15 
releaser: releaser_1.wav releaser_2.wav releaser_3.wav 15 
outernoise: { range: 350 soundmain: runningnoise.wav }
endsounds

internaldata:
fadesound: 5267_hasler-tykanie_1.wav
buzzer: sm42czuwak.wav
tachoclock: { sound1: hasler_1_km.wav sound2: hasler_2_km.wav sound3: hasler_3_km.wav sound4: hasler_4_km.wav sound5: 20786_hasler_5km.wav sound10: 20786_hasler_10_km.wav sound20: 20786_hasler_20_km.wav sound30: 20786_hasler_30_km.wav sound40: 20786_hasler_40_km.wav sound50: 20786_hasler_50_km.wav  sound60: 20786_hasler_60_km.wav sound70: 20786_hasler_70_km.wav sound80: 20786_hasler_80_km.wav sound90: 20786_hasler_90_km.wav sound100: 20786_hasler_100_km.wav sound110: 20786_hasler_110_km.wav sound120: 20786_hasler_120_km.wav sound130: 20786_hasler_130_km.wav sound140: 20786_hasler_140_km.wav sound150: 20786_hasler_150_km.wav sound500: 20786_hasler_150_km.wav }
switch: sm42-przelacznik.wav
relay: 20786_6d_pneumatic_relay.wav
pneumaticrelay: sm42-rownaniecisnien.wav
couplerattach: couplerattach.wav
couplerdetach: couplerdetach.wav
ignition: { range: 150 soundmain: 697_sm42-start-v2.wav }
 radiostop: [ 24150_radmor_rs_sygnal.wav 697_radiostop.wav ]

brakesound: 697_brake.wav 1.0 0.0 1.5 0.2
slipperysound: brake-slipp.wav 2.0 0.2  
airsound:  [1007]fv4a_ham.wav 0.25 -0.01
airsound2: [1007]fv4a_luz.wav 0.05 -0.01
airsound3: [1007]fv4a_e.wav 0.25 -0.01
airsound4: { soundmain: [ [1007]fv4a_x.wav 20786_et22_popelnianie.wav ] amplitudeoffset: -0.01 }
airsound5: [1007]fv4a_t.wav 10.0 -0.01
runningnoise: { range: -1 amplitudefactor: 0.4 soundmain: runningnoise.wav }

mechspring: 200 0.02 0.2 0.2 0.03 0.15 0.02 0.01
enginespring: 2.0 200 0.3 600 0.1

jointcabs: true

cab1definition:   
-1.65 1.8 -3.4 1.65 1.7 -2.3
driver1pos:
0.99 3.454 -3.311
driver1sitpos:   
-1.15 3.58 -2.83
cab1model: 6da_kabina.t3d

cab2definition:
-1.65 1.8 -3.4 1.65 1.7 -2.3
driver2pos:
-0.99 3.454 -3.311
driver2sitpos:   
1.15 3.58 -2.83
cab2model: 6da_kabina.t3d

mainctrl: { nastawnik rot -0.018 0.0 -0.05 sound0: 20786_control_6d_0.wav sound1: 20786_control_6d_1.wav sound2: 20786_control_6d_2.wav sound3: 20786_control_6d_3.wav sound4: 20786_control_6d_5.wav sound5: 20786_control_6d_6.wav sound6: 20786_control_6d_7.wav sound7: 20786_control_6d_3.wav sound8: 20786_control_6d_1.wav sound9: 20786_control_6d_5.wav sound10: 20786_control_6d_2.wav sound11: 20786_control_6d_6.wav }
scndctrl: { zbijacz04 mov -0.003 0 0.2 soundinc: 20786_203E_button_strong_reset_ca_shp_2_on.wav sounddec: 20786_203E_button_strong_reset_ca_shp_2_of.wav }
dirkey: { kier rot -0.09 0.01 0.15 soundinc: 20786_reverser_6d_inc_v2.wav sounddec: 20786_reverser_6d_dec_v1.wav sound0: 20786_reverser_6d_inc_v1.wav }
brakectrl: { zasadniczy rot 0.073 0.0 0.15 sound-2: 20786_203E_nast_ham_odc_1.wav sound-1: 20786_203E_nast_ham_pop_1.wav sound0: 20786_203E_nast_ham_0_4.wav sound1: 20786_203E_nast_ham_1_1.wav sound4: 20786_203E_nast_ham_2_1.wav sound5: 20786_203E_nast_ham_3_1.wav sound6: 20786_203E_nast_ham_nag_1.wav }
localbrake: { pomocniczy rot 0.019 0.0 0.3 soundinc: 20786_203e_additional_brake_1.wav sounddec: 20786_203e_additional_unbrake_1.wav sound0: 20786_manual_brake_6d_dec_0.wav sound10: 20786_manual_brake_6d_inc_10.wav }

fuse_bt: { przodreflprawy03 rot -0.2 0 0.2 soundinc: 20786_203E_switch_panto_3_on.wav sounddec: 20786_203E_switch_panto_3_of.wav }
instrumentlight_sw: { przodreflprawy24 rot -0.2 0 0.2 soundinc: 20786_203E_switch_light_devices_3_on.wav sounddec: 20786_203E_switch_light_devices_3_of.wav }
main_off_bt: { stop mov -0.003 0 0.2 soundinc: 20786_203E_button_ws_of_2_on.wav sounddec: 20786_203E_button_ws_of_2_of.wav }
main_on_bt: { start mov -0.003 0 0.2 soundinc: 20786_203E_button_ws_1_on.wav sounddec: 20786_203E_button_ws_1_of.wav }
security_reset_bt: { czuw_shp mov -0.003 0 0.2 soundinc: 20786_203E_button_strong_reset_ca_shp_2_on.wav sounddec: 20786_203E_button_strong_reset_ca_shp_2_of.wav }
releaser_bt: { odl mov -0.003 0 0.25 soundinc: 20786_203E_button_releaser_2_on.wav sounddec: 20786_203E_button_releaser_2_of.wav }
antislip_bt: { pposlz mov -0.003 0 0.2 soundinc: 20786_203E_button_ham_antyposlizgowy_2_on.wav sounddec: 20786_203E_button_ham_antyposlizgowy_2_of.wav }
upperlight_sw: { przodreflgora rot -0.2 0 0.2 soundinc: 20786_203E_switch_up_white_light_3_on.wav sounddec: 20786_203E_switch_up_white_light_3_of.wav }
leftlight_sw: { przodrefllewy rot -0.2 0 0.2 soundinc: 20786_203E_switch_left_white_light_2_on.wav sounddec: 20786_203E_switch_left_white_light_2_of.wav }
rightlight_sw: { przodreflprawy rot -0.2 0 0.2 soundinc: 20786_203E_switch_right_white_light_2_on.wav sounddec: 20786_203E_switch_right_white_light_2_of.wav }
leftend_sw: { przodczerwlewy rot -0.2 0 0.2 soundinc: 20786_203E_switch_panto_3_on.wav sounddec: 20786_203E_switch_panto_3_of.wav }
rightend_sw: { przodczerwprawy rot -0.2 0 0.2 soundinc: 20786_203E_switch_compressor_2_on.wav sounddec: 20786_203E_switch_compressor_2_of.wav }
rearupperlight_sw: { tylreflgora rot -0.2 0 0.2 soundinc: 20786_203E_switch_up_white_light_3_on.wav sounddec: 20786_203E_switch_up_white_light_3_of.wav }
rearleftlight_sw: { tylrefllewy rot -0.2 0 0.2 soundinc: 20786_203E_switch_left_white_light_2_on.wav sounddec: 20786_203E_switch_left_white_light_2_of.wav }
rearrightlight_sw: { tylreflprawy rot -0.2 0 0.2 soundinc: 20786_203E_switch_right_white_light_2_on.wav sounddec: 20786_203E_switch_right_white_light_2_of.wav }
rearleftend_sw: { tylczerwlewy rot -0.2 0 0.2 soundinc: 20786_203E_switch_panto_3_on.wav sounddec: 20786_203E_switch_panto_3_of.wav }
rearrightend_sw: { tylczerwprawy rot -0.2 0 0.2 soundinc: 20786_203E_switch_compressor_2_on.wav sounddec: 20786_203E_switch_compressor_2_of.wav }
horn_bt: { horn rot -0.05 0 0.05 soundinc: 20786_203E_switch_horn_pom_high_3_on.wav sounddec: 20786_203E_switch_horn_pom_high_3_of.wav }
cablight_sw: { przodreflprawy22 rot -0.2 0 0.2 soundinc: 20786_203E_switch_lights_cabin_2_on.wav sounddec: 20786_203E_switch_lights_cabin_2_of.wav }
fuelpump_sw: { pompka_paliwa rot -0.2 0 0.2 soundinc: 20786_203E_switch_lights_cabin_2_on.wav sounddec: 20786_203E_switch_lights_cabin_2_of.wav }
dimheadlights_sw: { box06 rot -0.2 0 0.2 soundinc: 20786_203E_switch_lights_cabin_2_on.wav sounddec: 20786_203E_switch_lights_cabin_2_of.wav }
maxcurrent_sw: { prz02 rot 0.25 0 0.2 soundinc: 20786_203e_przel_pakiet_6.wav sounddec: 20786_203e_przel_pakiet_4.wav }
brakeprofileg_sw: { przodreflprawy09 rot -0.2 0 0.2 soundinc: 20786_203E_switch_compressor_2_on.wav sounddec: 20786_203E_switch_compressor_2_of.wav }
oilpump_sw: { przodreflprawy17 rot -0.2 0 0.2 soundinc: 20786_203E_switch_lights_cabin_2_on.wav sounddec: 20786_203E_switch_lights_cabin_2_of.wav }
waterheater_sw: { box03 rot -0.2 0 0.2 soundinc: 20786_203E_switch_lights_cabin_2_on.wav sounddec: 20786_203E_switch_lights_cabin_2_of.wav }
radiochannel_sw: { swr-kanal rot -0.085 0 0.1 soundinc: [ 20786_radmor_pokretlo1.wav 20786_radmor_pokretlo2.wav 20786_radmor_pokretlo3.wav 20786_radmor_pokretlo4.wav 20786_radmor_pokretlo5.wav ] sounddec: [ 20786_radmor_pokretlo1.wav 20786_radmor_pokretlo2.wav 20786_radmor_pokretlo3.wav 20786_radmor_pokretlo4.wav 20786_radmor_pokretlo5.wav ] }
radiostop_sw: radiostop mov -0.005 0 0
radio_sw: { swr-wl mov -0.004 0 0.002 soundinc: 20786_203e_button_radio_3_on.wav sounddec: 20786_203e_button_radio_3_of.wav }
shuntmodepower: regulator rot -0.77 0 0.1
tachometer: speedknob rot 0.00635 0.0 0
Hvoltage: miernik3 mov 0.00009 0 1
HVcurrent1: miernik4 mov 0.00005 0 1
enrot1m: obrot rot 0.027 0 0.3
enrot2m: obrot01 rot 0.027 0 0.3
brakepress: cyl06 rot 0.71 0 0
pipepress: cyl03 rot 0.715 0 0
compressor: cyl02 rot 0.4576 0 0
compressorb: cyl01 rot 0.4576 0 0
oilpress: cyl04 rot -0.55 -0.0333 0.0
oiltemp: cyl05 rotvar -0.00025 -0.046 0.1 100 -0.0046
water1temp: cyl07 rotvar -0.00025 -0.05 0.1 100 -0.0046
clock: analog 

i-scnd1: bocznikowanie
i-instrumentlight: podswietlenie
i-motor_ovld: nadmiar
i-security_aware: czuwak
i-radio: rtf
i-malfunction: awaria
i-malfunctionb: uszk_lok_ster

cab0definition:
-1.1 1.5 6.57 1.1 1.5 6.6
driver0pos:
0.0 2.21 -6.55
cab0model: none