models: 6dg.t3d
animations: 4 0 0 4 2 0 -1
lowpolyinterior: lowpoly.t3d
animwheelprefix: wheel0
endmodels

locations:
 tractionmotors: -3.736 3.788 end
 bogies: -3.736 3.788 end
endlocations

sounds:
wheel_clatter: 70 -5.044 wheel-heavy.wav -2.444 wheel-heavy.wav 2.426 wheel-heavy.wav 5.026 wheel-heavy.wav end
engine: {
 amplitudefactor: 0.9
 amplitudeoffset: 1.25
 range: 150
 crossfade: 90
 sound580: 697_6dg-low.wav pitch580: 1
 sound1100: 697_6dg-medium.wav pitch1100: 1.65
 sound1850: 697_6dg-high.wav pitch1850: 1.875
 soundend: 697_6dg-stop.wav }
tractionmotor: 697_st44-motor.wav 20.0  1.5 0.8  0.16 0.1
brake: 697_sm42_brake.wav 100.0 1700.0 -1.0
derail: derail.wav 200
horn1: 6dg_rp1_1_start.wav 6dg_rp1_1_trwa.wav 6dg_rp1_1_stop.wav 400
horn2: 6dg_rp1_2_start.wav 6dg_rp1_2_trwa.wav 6dg_rp1_2_stop.wav 600
turbo: turbo-m.wav turbo-m.wav turbo-m.wav 150
sand: sand_1.wav sand_2.wav sand_3.wav 15 
releaser: releaser_1.wav releaser_2.wav releaser_3.wav 15 
outernoise: { range: 350 soundmain: runningnoise.wav }
endsounds 

internaldata:
buzzer: bzyczek2k.wav
pneumaticrelay: pneumaticrelay.wav
 couplerattach: [ couplerattach.wav 697_hak_zakladanie.wav ]
 couplerdetach: [ couplerdetach.wav 24150_pg_otwarcie_kurka.wav ]
ignition: { soundmain: 697_6dg-start.wav range: 150 }
radiostop: 24150_koliber_rs_sygnal.wav
brakesound: 697_brake.wav 1.0 0.0 1.5 0.2
slipperysound: brake-slipp.wav 2.0 0.2
airsound:  { soundmain: [ 697_fv4a_syk.wav 697_ep05-hiss.wav sm42-powietrze.wav 07]hiss.wav ] amplitudeoffset: -0.01 }
airsound2: [1007]fv4a_luz.wav 0.05 -0.01
airsound3: [1007]fv4a_e.wav 0.25 -0.01
airsound4: { soundmain: [ [1007]fv4a_x.wav 20786_et22_popelnianie.wav ] amplitudeoffset: -0.01 }
airsound5: [1007]fv4a_t.wav 10.0 -0.01
runningnoise: { range: -1 amplitudefactor: 0.4 soundmain: runningnoise.wav }

mechspring: 100 0.02 0.2 0.2 0.03 0.15 0.02 0.01
enginespring: 1.5 100 0.3 800 0.4

jointcabs: true

cab1definition:
-1.73 1.7 -3.7 1.73 1.7 -2.3
driver1pos:
-1.08 3.69 -3.47
driver1sitpos:
-1.17 3.37 -2.9
cab1model: 6dg_1]kabina_a.t3d

cab2definition:   
-1.73 1.7 -3.3 1.73 1.7 -2.0
driver2pos:
1.1 3.47 -2.1
driver2sitpos:
1.17 3.37 -2.8
cab2model: 6dg_1]kabina_b.t3d  

battery_sw: { aktywacja rot -0.1 0 0.1 soundinc: 20786_104e_switch_lights__2.wav sounddec: 20786_104e_switch_lights_3.wav }
mainctrl: { nastawnik rot -0.00667 0.0 0.2 soundinc: 20786_traxx_little_silence.wav sounddec: 20786_traxx_little_silence.wav sound21: 20786_traxx_control_inc.wav sound0: 20786_traxx__control_dec.wav }
dirkey: { kier rot 0.02 0.01 0.15 soundinc: 20786_203e_hebelek_3_on sounddec: 20786_203e_hebelek_3_of.wav }
brakectrl: { zasadniczy rot -0.04 0 0.2 sound-2: 20786_189_brake_7.wav sound-1: 20786_189_unbrake.wav sound0: 20786_189_brake_1.wav sound1: 20786_189_brake_2.wav sound2: 20786_189_brake_3.wav sound3: 20786_189_brake_4.wav sound4: 20786_189_brake_5.wav sound5: 20786_189_brake_6.wav sound6: 20786_189_emergency_brake.wav }
localbrake: { pomocniczy rot 0.014 0 0.2 soundinc: 20786_traxx_little_silence.wav sounddec: 20786_traxx_little_silence.wav sound10: 20786_traxx_control_inc.wav sound0: 20786_traxx__control_dec.wav }
brakeprofile_sw: { towos rot 0.2 0 0.2 soundinc: 20786_ep09_switch_on.wav sounddec: 20786_ep09_switch_of.wav }
main_off_bt: { stop mov -0.003 0 0.2 soundinc: 20786_203e_button_1_on.wav sounddec: 20786_203e_button_1_of.wav }
main_on_bt: { start  mov -0.003 0 0.2 soundinc: 20786_203e_button_3_on.wav sounddec: 20786_203e_button_3_of.wav }
security_reset_bt: { czuw_shp mov -0.003 0 0.2 soundinc: 20786_203e_big_button_3_on.wav sounddec: 20786_203e_big_button_3_of.wav }
releaser_bt: { odluzniacz mov -0.003 0 0.2 soundinc: 20786_203e_button_2_on.wav sounddec: 20786_203e_button_2_of.wav }
antislip_bt: { pposlz mov -0.003 0 0.2 soundinc: 20786_203e_button_6_on.wav sounddec: 20786_203e_button_6_of.wav }
tachometern: wskpr rot 0.005 0.0 0.2
instrumentlight_sw: { podswietlenie rot -0.1 0 0.1 soundinc: 20786_104e_switch_lights.wav sounddec: 20786_104e_switch_lights_3.wav }
cablight_sw: { oswietlenie rot -0.1 0 0.1 soundinc: 20786_104e_switch_lights.wav sounddec: 20786_104e_switch_lights_3.wav }
hvoltage: Plane12 mov 0.00009 0 1
hVcurrent1: Plane11 mov 0.00004 0 1
enrot1m: obrot mov 0.002 0 0.3
brakepress: cyl06 rot 0.73 0 0
pipepress: cyl03 rot 0.73 0 0
compressor: cyl02 rot 0.4576 0 0
dimheadlights_sw: { przyciemnienie_reflektorow rot 0.1 0 0.1 soundinc: 20786_104e_switch_lights.wav sounddec: 20786_104e_switch_lights__2.wav }
clock: analog
radiochannelprev_sw: { klawisz_4 rot 0 0 0 soundinc: 24150_koliber_klik.wav }
radiochannelnext_sw: { klawisz_6 rot 0 0 0 soundinc: 24150_koliber_klik.wav }
radiostop_sw: { radiostop_off mov -0.001 0 0 soundinc: 24150_koliber_rs_wcisniecie.wav sounddec: 24150_koliber_rs_puszczenie.wav }
radio_sw: { klawisz_potw rot 0 0 0 soundinc: 24150_koliber_klik.wav sounddec: silence1.wav }
lights_sw: { swiatla rot 0.13 0 0.1 soundinc: 20786_104e_switch_lights.wav sounddec: 20786_104e_switch_lights_3.wav }
horn_bt: { horn rot -0.05 0 0.05 soundinc: 20786_203e_hebelek_1_on sounddec: 20786_203e_hebelek_1_of.wav }
alarmchain: { hamulec_bezpieczenstwa rot -0.25 0 0.25 soundinc: [1007]fvel6_brake_1.wav sounddec: 20786_189_unbrake.wav }

i-slippery: poslizg
i-security_aware: czuwak
i-security_cabsignal: shp
i-instrumentlight: podswietlenie
i-door_left: informacje
i-forward: kierunek
i-backward: kierunek_tyl
i-radiostop: radiostop
i-upperlight: upper
i-leftlight: left 
i-rightlight: right
i-leftend: leftend
i-rightend:	rightend
i-rearupperlight: rearupper
i-rearleftlight: rearleft
i-rearrightlight: rearright
i-rearleftend: rearleftend
i-rearrightend: rearrightend
i-radio: { radio soundinc: 24150_koliber_start.wav sounddec: 24150_koliber_wylaczenie.wav }

cab0definition:
-1.1 1.8 -3.2 1.1 1.7 -2.3
driver0pos:
0.0 3.5 -3.1
cab0model: none

pyscreen: ekran_wlaczony koliber_hasler_elektroniczny