Param. Category=train M=35500 Vmax=110 PWR=0 SandCap=0 Type=ezt
Load: MaxLoad=54 LoadQ=pieces LoadAccepted=Passengers,Pantstate OverLoadFactor=2 LoadSpeed=1 UnLoadSpeed=1
Dimensions: L=20.87 H=4 W=2.9 Cx=0.2 
Wheels: D=0.94 AIM=2000 Tw=1.435 Axle=2'2' Ad=2.83 Bd=13.9 Rmin=80 BearingType=Roll
Brake: BrakeType=Oerlikon BrakeValve=EP2 NBpA=4 MBF=85.0 MaxBP=0.4 BCN=1 BCR=0.2 BCD=0.15 BCM=8 HiPP=0.5 LoPP=0.34 Vv=0.3 MinCP=0.58 MaxCP=0.72 CompressorSpeed=0.013
Doors: OpenCtrl=DriverCtrl CloseCtrl=DriverCtrl OpenSpeed=0.2 CloseSpeed=0.1 DoorMaxShiftL=0.32 DoorMaxShiftR=0.27 DoorOpenMethod=Shift DoorClosureWarning=Yes 
BuffCoupl. CType=Automatic kB=4200 DmaxB=0.05 FmaxB=1740 kC=6800 DmaxC=0.15 FmaxC=780 beta=0.58
Cntrl. BrakeSystem=ElectroPneumatic BrakeHandle=FVel2  BCPN=4 BDelay1=15 BDelay2=4 ASB=Manual LocalBrake=ManualBrake DynamicBrake=Passive MCPN=3  SCPN=3 IniCDelay=0.0 SCDelay=0.8 CoupledCtrl=Yes
-1 0.5 	0.0	6  ElectroPneumatic
 0 -1	-1	0  ElectroPneumatic
 1 -1   0.35	4  ElectroPneumatic
 2 -1   -1      0  Pneumatic
 3 0.34	-1	2  Pneumatic
 4 0	-1	40 Pneumatic
Security: AwareSystem=Active,CabSignal AwareDelay=60 SoundSignalDelay=5 EmergencyBrakeDelay=6 RadioStop=Yes 
Light: Light=Generator LGeneratorEngine=ElectricSeriesMotor LMaxVoltage=110 LMaxCurrent=155  
Power: EnginePower=CurrentCollector CollectorsNo=2 MaxVoltage=3600 MaxCurrent=1200 MinH=0.38 MaxH=2.4 CSW=1.4
Switches: Pantograph=impulse Converter=impulse
