# prametry hamulca dla SPKS: youBy
Param. Category=train M=42200 Vmax=120 HeatingP=40 LightP=0.56
Load: MaxLoad=132 LoadQ=pieces LoadAccepted=Passengers,Luggage OverLoadFactor=2 LoadSpeed=1 UnLoadSpeed=2
Dimensions: L=26.8 H=4.7 W=2.88 Cx=0.15
Wheels: D=0.96 Tw=1.435 Axle=2'2' Ad=2.5 Bd=19.5 Rmin=80 BearingType=Roll
Brake: BrakeValve=KE NBpA=6 MBF=15 MaxBP=3.8 BCN=12 BCR=0.127 BCD=0.04 BCM=1.5 BCS=1.2 BSA=0 BM=Disk1 BVV=125 TareMaxBP=2.3
Doors: OpenCtrl=Passenger CloseCtrl=Mixed OpenSpeed=0.5 CloseSpeed=0.4 DoorMaxShiftL=0.4 DoorMaxShiftR=0.4 DoorOpenMethod=Shift DoorClosureWarning=Yes 
BuffCoupl. CType=Screw kB=9200 DmaxB=0.11 FmaxB=320 kC=4500 DmaxC=0.1 FmaxC=850 beta=0.58 AllowedFlag=115
Cntrl. BrakeSystem=Pneumatic LocalBrake=ManualBrake BrakeDelays=P MaxBPMass=63
Light: Light=Generator LGeneratorEngine=WheelsDriven LMaxVoltage=24 AlterLight=Accu AlterLMaxVoltage=24 AlterLCap=495 AlterLRS=Generator 
Clima: Heating=PowerCable HPowerTrans=ElectricPower HMaxVoltage=3000 AlterHeating=PowerCable AlterHPowerTrans=SteamPower AlterHSteamPress=0.45