models: bdhpumn.t3d
animations: 4 4 0 4 2 0 -1
lowpolyinterior: wnetrze_ng.t3d
animwheelprefix: wheel0
animdoorprefix: door0
endmodels

locations:
doors: -6.30 both 6.30 both end
bogies: -10.85 10.85  end
endlocations

sounds:
curve: { amplitudefactor: 1.35 amplitudeoffset: 1.35 range: 100 crossfade: 75 sound1: 20786_curve_111a.wav sound10: 20786_curve_111a.wav sound40: 20786_curve_111a.wav sound50: 20786_curve_111a.wav sound60: 697_et22_curve.wav sound80: silence1.wav }
outernoise: { range: 90 amplitudefactor: 1.7 amplitudeoffset: 0.2 crossfade: 90
sound0: cisza.wav pitch1: 1
sound1: 1xxa-5.wav pitch1: 1
sound17: 1xxa-17_3.wav pitch1: 1
sound20: 1xxa-23.wav pitch1: 1
sound35: 1xxa-35_4.wav pitch1: 1
sound63: 1xxa-63_3.wav pitch1: 1
sound80: 1xxa-80.wav pitch1: 1
sound100: 1xxa-100.wav pitch1: 1
sound120: 1xxa-120.wav pitch1: 1
sound190: 1xxa-120.wav pitch1: 1 }
wheel_clatter: 50.0 11.0 20786_kolo_bautzen_1.wav 8.47 20786_kolo_bautzen_2.wav  -8.47 20786_kolo_bautzen_3.wav -11.0 20786_kolo_bautzen_4.wav  end
brake: [20786_Brake_bmnopux.wav 50.0 800.0 -1.0
derail: derail.wav 200
unbrake: [1007]estluz.wav 50
brakeacc: { soundmain: [ brakeacc_est3f.wav [1007]est_bac.wav ] range: 50 }
releaser: releaser_1.wav releaser_2.wav releaser_3.wav 15 
dooropen: [20786_Door_open_Bmnopux_1.wav
doorclose: [20786_Door_close_automatic_Bmnopux_1.wav
unloading: [ passengers_loading_1.wav passengers_loading_2.wav ]
loading: [ passengers_loading_1.wav passengers_loading_2.wav ]
endsounds 

internaldata:
runningnoise: [20786_runningnoise_Bmnopux_2.WAV 1.2 0.4 1 0.05   
  couplerattach: [ couplerattach.wav couplerattach_default.wav ]
  couplerdetach: [ couplerdetach.wav couplerdetach_default.wav ]
  brakehoseattach: hoseattach.wav  // przewod glowny hamulca zapiecie
  brakehosedetach: hosedetach.wav  // przewod glowny hamulca rozpiecie
  mainhoseattach: hoseattach.wav  // przewod zasilajacy zapiecie
  mainhosedetach: hosedetach.wav  // przewod zasilajacy rozpiecie
  controlattach: controldetach.wav // ukrotnienie zapiecie
  controldetach: controldetach.wav // ukrotnienie rozpiecie
  gangwayattach: gangwaydetach.wav // mostek zapiecie
  gengwaydetach: gengwaydetach.wav // mostek rozpiecie
  heatingattach: heatingdetach.wav // ogrzewanie zapiecie
  heatingdetach: heatingdetach.wav // ogrzewanie rozpiecie

mechspring: 210      0.08 0.371 0.1 0.01 0.10  0.02   0.01

cab1definition:
-1.2 0.446 -5.035 1.2 2.563 5.035
driver1pos:
-0.968 1.515 0.7
cab1model: wnetrze_ng.t3d

cab2definition:
-1.2 2.635 -6.7 1.2 4.417 6.7
driver2pos:
-0.57 3.798 1.486
cab2model: wnetrze_ng.t3d

cab0definition:
-1.2 1.1 7.829 1.2 3.313 11.2
driver0pos:
-0.5 2.279 9.962
cab0model: wnetrze_ng.t3d